Lab 1: Below you are tasked with dragging the MOST APPROPRIATE Cable to the most appropriate device termination.

Instructions: Controls can be used more than one time and not all options will be used. In this scenario, a switch only works at Layer 2

Crossover  
Cable

RS-232

RS-232

RS-232

Computer to computer

RG-8

RG-8

RG-8

RG-6

RG-6

RG-6

Switch to Hub

Hub to Repeater

Computer to Router

Console Port of router

Router to Hub

Switch to computer

Rollover Cable

Rollover Cable

Rollover Cable

Rollover Cable

Straight Thru Cable

Straight Thru Cable

Straight Thru Cable

Straight Thru Cable

Crossover  
Cable

Crossover  
Cable

Crossover  
Cable

H.323

H.323

H.323

Switch to Switch

H.323